Important information on the 2.0.2X firmware and RIP version 1.03 for PC and 1.02 for Palm

*****IMPORTANT*****

Firmware 2.0.25 contains new firing modes called Hypermode and 3 shot burst - Please note that 
these modes are NOT considered torunament legal and they should only be used on fields where 
non semi modes are allowed.

Also please note that these two new modes are to be considered as full auto modes and therefore 
they might be illegal in your country of residence - please check before using these modes.

Racegun is not in any way responsible for your use of these modes and we recommend that if you 
are in doubt you should not use these new modes.

Firmware 2.0.26 is a semi only firmware (supports only semi and classic mode) - Racegun recommends that this firmware is used by anyone playing on the tournament circuit.


Changes to the new firmwares:
New modes added (3 shot burst and Hyper mode)
Special tournament (semi only version) released separately
CTO adjust reversed (the manual is now correct - CTO adjust is enabled when RIP tickbox is checked)
Triggerfilter unchecked in semimode no longer fires the grip in autoresponse mode
EYE logic changed for faster ACE functionality
EYE check max and EYE OK max - values now set
Timer is tunred off (when beeping) by pressing arrow down 
Other minor undisclosed changes  

Changes to new RIP's (Both PC and Palm version):
Added window with notification when using full auto, Hyper and burst mode
Added support for new modes
General minor clean ups

PLEASE READ THE ATTACHED "RIP SOFTWARE GUIDE" BEFORE USING THE NEW FIRMWARE/SOFTWARE

*****LIMITATIONS*****

The new firmwares does not support 9 volt operation (for 9 volt grips use firmware version 2.0.5)
The new Firing modes will only work with firmware version 2.0.23
If you are using firmware 2.0.24 or 2.0.26 you can only use Semi and classic mode any other selection will put the grip into classic mode.
Palm RIP does not support 9 volt grips
Palm RIP does not support "putting" of firmware to the grip


